EAW's PLM Series preset for EAW's JFL speaker.

JFL210x4-6 Bi-amp w/ Sub High Pass Filter

Application Notes:
JFL210 is high-passed at 100 Hz with 24 dB Linkwitz-Riley for 
use with subwoofer. Use with an array of four to six JFL210. 
DSP settings are equivalent to single-amp Multi Box mode. 

To approximate Single Box and/or Long Throw modes insert the 
following filters in the Input PEQ:

* Single Box: 5 kHz, -3.0 dB, 1.33 BW
* Long Throw: 10 kHz, +3.0 dB, 1.60 BW

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.