Lab.gruppen's PLM Series preset suitable for L-Acoustics' SB28 speaker.

Application notes:
The preset is low-passed at 60 Hz, for use in combination with e.g. 
KUDO or V-DOSC systems.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay, when using the channel SB28 3.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10 dBu (SUB)
* ISVPL threshold at 173.7 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +15 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk