Lake XP preset for ADAMSON IS10p 100x50
========================

Application Notes:
     - Fullrange Mode
     - Linear Phase response matching all E-, S- and IS-Series Line Source and Point Source when positioned in the same distance including linear phase latency
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 1
     - Module out 2 - HF: Ch. 2

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2

