Adamson's preset for Adamson's SpekTrix speaker Under Hang E-Series


Application Notes:
     Linear Phase Preset
     The preset is high-passed at 110 Hz
     Maximum of 4 cabinets in parallel per amplifier.

     IF USED WITH LM26 beside PLMs add 0.63ms as outputs delay.

Routing:
     Ch1 : Free
     LF : 2
     MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     SpekTrix v1.0b BETA
     Beta fingerprints may produce incorrect results

Designed by DV2
Didier DAL FITTO
Daniel Grubac