*** TURBOSOUND BERLIN TBV Series ***
____________________________________________________

TBV118L 1-WAY 80 Hz CARDIOID module

OUTPUTS: Ch1 = TBV118L REAR-FIRING SUB (80 Hz LPF)

Pre-aligned for use with TBV118L FRONT-FIRING enclosures
when processed with "TBV118L 1W 80 Hz" modules

RECOMMENDED 2:1 RATIO for FRONT-FIRING : CARDIOID (rear-firing) 
TBV118L enclosures for optimum rear rejection
____________________________________________________

EQ OVERLAYS:

- LT COMPENSATION  

Notes:
 
1) insert LT COMPENSATION to maintain tonal balance
consistency when LT overlay is inserted in
"TBV123 2W FULLRANGE" or "TBV123 PASSIVE FULLRANGE" modules
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TBV QSG and Rigging Manual prior to use 

*** Designed by Music Group - 31 MAR 2017 ***
http://www.music-group.com/support/