Lake FIR preset for ADAMSON S10n
=========================

Application Notes:
     - Default LF compensation for 5 to 6 cabinets per array
     - All modules in the array need to use the same preset
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 2 - LF: Ch. 3 / 1 with pin swap cable
     - Module out 3 - HF: Ch. 4 / 2 with pin swap cable

Technical Info:
     - Fingerprint: V3.0

=======================
Designed by ADAMSON & DV2