EAW's PLM Series preset for EAW's MW speaker
 
MW12 Bi-amp Full Range

Application Notes:
MW12 is high-passed at 60 Hz with 18 dB Butterworth filter for 
full range operation.

"GREY" Setting: EQ slope is -1 dB per octave (constant slope) in 
half-space conditions.

Technical info:
Factory output gains assume amplifiers for each passband have the same voltage gain.
If voltage gains of amplifiers in use do not match, see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.
Attack/release times are optimized for each passband.

Fingerprint: MW12 v1.0b2 BETA
Beta fingerprints may produce incorrect results.