*** Tannoy AMS Series ***
___________________________________________

PLM & LM Series preset for Tannoy AMS Series
Products utilised in LOW Z mode or in 100V mode


AMS5DC, AMS6DC, AMS8DC
AMS5ICT, AMS6IST
___________________________________________

Application Notes:

This 3 AUX module has 3 Processed outputs:

1 = FLAT : Fullrange Settings
2 = CUT  : 120Hz LF Cut (For use either standalone or with Sub)
3 = SUB  : Matched Sub output for use with the above CUT output

This module can be used in combination with VSX Sub Module Files
should a different combination other than the one 
supplied be required.
___________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***

::: Thomas Vestergaard :::
