Lake preset for ADAMSON P12 Passive
===============================

Application Notes:
     - For Standard Waveguide 60x40
     - BRIGHT EQ curve for wedge monitor position
     - Fullrange Mode
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - FR
     - Module out 2 - FR

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2