Lab.gruppen's PLM Series preset suitable for L-Acoustics' ARCS speaker.

Application notes:
Created for the "ARCS 2W LO" application; 
ARCS 2-way preset,  nominal flat (freefield) with normal HF shelving eq.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), +2 dBu (HF)
* ISVPL threshold at 137.8 Vpk (LF), 69.1 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (LF), +7 dBu-pk (HF)

Fingerprint info:
ARCS v1.0 beta1