MDC12 Mesa EQ Mode

Application Notes:
     Passive Mode
     FOH position
     Xover frequency : 100Hz

Routing:


Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME