EV's PLM Series preset suitable for EV's X-LINE System.

Application Notes:
EV X-Sub to be used with XVLS & XVLT (33Hz - 80Hz)

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.
The sub to top ratio is set to 1:1.
Subwoofers are time-aligned and level adjusted to be flown in the 
same array, or in an array directly next to the main X-Line hang.
Output levels and delay settings will need to change if Xsub is 
used with systems other than X-Line.

EV Rev Number: Version 4 (Standart Preset)
Dolby Lake Rev Number: Version 1

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (SUB) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
