EAW's PLM Series preset for EAW's KF speaker
 
KF750 Settings for 1 Row KF750/1 Row KF755 Array, Tri-amp w/ Sub High Pass Filter

Application Notes:
KF750 is high-passed at 80 Hz with 24 dB Linkwitz-Riley filter for 
use with subwoofer. Use in conjunction with "1x KF755w750 TRI_SubHPF" 
settings for complete array processing. 

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.