EAW's PLM Series preset for EAW's JFL speaker.

JFL210x1 Bi-amp "Near" Full Range

Application Notes:
JFL210 is high-passed at 60 Hz with a 12 dB Butterworth filter for 
full range operation. Use preset with a single JFL210 for front 
or side fill applications where typical listener distances are <2 meters.

Technical info:
Factory output gains assume amplifiers for each passband have 
the same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.