*** TURBOSOUND NuQ Series
*** NuQ62, NuQ81, NuQ102, NuQ122, NuQ152, NuQ115B, NuQ118B
____________________________________________________

PLM & LM series modules:

Amplifier GAIN is 35dB - within PLM & D Series this is locked 
& preset in the module.

For use with LM controllers and other amplifiers please set 
the amplifier input gain to 35dB failure to do this could
result is poor performance or damage to the system!

____________________________________________________

These models have 1, 2 or 3 processed output channels:
FR = Full Range (1 Channel)
FR + Sub = Full Range and Subwoofer (2 Channels)
Bi-amp Full Range (2 Channels)
Bi-amp + Sub (3 Channels)

There are 2 modules for each Subwoofer:
'H' = crossover at 120 Hz
'L' = crossover at 100 Hz

NuQ82, NuQ102 crosses over with NuQ115B at 120Hz as standard
NuQ122, NuQ152 crosses over with NuQ118B at 100Hz as standard
____________________________________________________

Routing:

Any channel can be routed to the required output
from these modules.

WARNING: Ensure correct routing before use.
____________________________________________________      

*** Designed by Music Group ***

::: V001 Andrew Pardoe 30/08/2016 :::