*** TURBOSOUND TQ Series & Lab Gruppen IPX4800               ***
***       V1.0 FIR-X RELEASE                                 ***
*** All PRESETS CREATED IN IPX CONTROLLER V2.3.4             ***
*** All PRESETS ONLY FOR IPX4800                             ***
***         README                                           ***

IPX1200 & IPX2400 ARE NOT SUPPORTED!

SOME OF THE NAMING CONVENTION FROM LAKE PLM PRESETS IS SHORTENED AS THE IPX NAMING WINDOW HAS LESS CHARACTERS AVAILABLE!

TERMS:

HR = HORN ROTATED
FR = FULL RANGE WITHOUT SUBWOOFER
FR HR = FULL RANGE WITHOUT SUBWOOFER, HORN ROTATED
CUT HR = HORN ROTATED, X-OVER HPF FOR TQ15B OR TQ18B SUBWOOFER
CUT = X-OVER HPF FOR TQ15B OR TQ18B SUBWOOFER
FB = CARDIOID, 1PCS OF SUBWOOFER FORWARD, 1PCS OF SUBWOOFER BACKWARDS
FFB = CARDIOID, 2PCS OF SUBWOOFER FORWARD, 1PCS OF SUBWOOFER BACKWARDS
REF = REVERSED END FIRE
TQxxB REF F.R 1ST CHANNEL IS FRONT, 2ND CHANNEL IS REAR, GAP IS 44CM BETWEEN REAR CABINET GRILLE AND FRONT CABINET REAR PANEL (where the wheel bolt on)
TQxxBCARD FB = 1ST CHANNEL IS FRONT/FORWARD, 2ND CHANNEL IS BACK/BACKWARDS
TQxxBCARD FFB = 1ST CHANNEL IS 2pcs FRONT/FORWARD, 2ND CHANNEL IS 1pcs BACK/BACKWARDS
TQxx CUT TQxxB = 1ST CHANNEL TQxx CUT (X_OVER HPF) 2ND CHANNEL TQxxB SUBWOOFER
TQxxM CUT TQxxB = 1ST CHANNEL TQxxM CUT (X_OVER HPF) 2ND CHANNEL TQxxB SUBWOOFER
TQxxM FR TQxxB = 1ST CHANNEL TQxxM FR (NO X_OVER HPF) 2ND CHANNEL TQxxB SUBWOOFER (OVERLAP 90-50Hz)

NOTES:
Output patch is fixed - sorry its not LAKE/PLM

IPX1200 & IPX2400 ARE NOT SUPPORTED!

POLARITY REVERSE ON INPUTS IS A REQUESTED FEATURE BY TURBOSOUND TO LAB GRUPPEN - WE AWAIT THE NEXT RELEASE FROM LAB GRUPPEN

ALIGNMENT LATENCY IS FOR IPX TO PLM FOR MIXED SYSTEMS, EXCEPT TQxxM Stage Monitors where a hydrid low latency approach is used

TQ12M/TQ14M STAGE MONITORS ARE A SEPERATE RELEASE FOLDER/BANK

MAXIMUM QTY OF SUBWOOFERS IS 2pcs PER CHANNEL (4 OHM LOAD)

MAXIMUM QTY OF FULL RANGE / STAGE MONITORS IS 2pcs PER CHANNEL (4 OHM LOAD)

LOAD 'FACTORY FILE' loads the complete bank of presets on to IPX4800

____________________________________________________


PLEASE CONSULT THE QUICK START GUIDE FOR DETAILED INSTRUCTIONS

____________________________________________________



*** Designed by TURBOSUND - DEC2024 ***
http://www.turbosound.com
