Martin Audio's Lab.gruppen PLM Series presets suitable for a Martin Audio system of 
W8L, W8LD and W8LS speakers.

Application notes:
Designed for a flown application of a number of W8L with W8LD as downfill together with 
W8LS subwoofers. Default delays are user editable to align the system further.

HiC and LoC in the folder names correspond to Hi Curve and Lo Curve applications.
HFB and HFN stands for High Frequency Boost and HF Normal, respectively. 

The "far", "mid" and "near" suffixes refer to different positions of the
flown speakers, from top to bottom in the array.

For a more detailed reference of the speaker setup, see the 
"W8L Series Detailed Applications Guide" on the Martin Audio website, www.martinaudio.com.