Seeburg Acoustic Line's PLM Series preset suitable for Seeburg's Galeo speaker.

Application notes:
Delay suitable for stacking on Galeo Sub

Created by Fabian Vuine, Seeburg Acoustic Line

Technical info:
* 32 dB Amp Gain 
* ISVPL threshold at 135.1 Vp (LF), 61.6 Vp (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)