Martin Audio's PLM Series preset suitable for Martin Audio's LE12J speaker.

Application notes:
The preset is designed for a monitor application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +0.0 dBu (LF), -0.5 dBu (HF)
* ISVPL threshold at 98.0 Vpk (LF), 57.0 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +10 dBu-pk (LF), +5 dBu-pk (HF)