DAS Audio's PLM Series preset suitable for DAS Audio's LX-218 speaker.

Application notes:
1+1 module created for the "LX-218" application. If used together with DAS AERO50, 
then use "DAS 8 AERO50 HP" or "DAS 12 AERO50 HP" 3-Way presets. 
Each of the 2 identical subwoofer channels has a separate input mixer 
to allow for a Left and Right subwoofer that only uses one module. 

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +7.0 dBu (SUB)
* MaxPeak limiter threshold at +10.0 dBu (SUB)
* ISVPL threshold at 138.0 Vpk (SUB)