Lab.gruppen's PLM Series preset suitable for JBL's VT4887A speaker.

Application notes:
The preset is a 2-way configuration, high-passed at 60 Hz, 
for short throw or distributed fill application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +11 dBu (LF), +5 dBu (MHF)
* ISVPL threshold at 154.8 Vpk (LF), 87.0 Vpk (MHF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +14 dBu-pk (LF), +9 dBu-pk (MHF)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk
* To emulate 26 dB Amp Gain - set input gain to -6 dB