Martin Audio's Lab.gruppen PLM Series presets suitable for a Martin Audio system of 
W8LM, WLX, WS218X and WMX speakers.

Application notes:
Designed for a flown application of a number of W8LM (with the possibility of 
using W8LMD as downfill with the same preset) together with a selection of 
subwoofers. Default delays are user editable to align the system further.

HiC and LoC in the folder names correspond to Hi Curve and Lo Curve applications.
HFB and HFN stands for High Frequency Boost and HF Normal, respectively. 

The "far", "mid" and "near" suffixes refer to different positions of the
flown speakers, from top to bottom in the array.

For a more detailed reference of the speaker setup, see the 
"W8L Series Detailed Applications Guide" on the Martin Audio website, www.martinaudio.com.