Lab.gruppen's PLM Series preset suitable for L-Acoustics' KARA speaker

Application notes:
The module file is a 2-way configuration, designed for a fill application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +4.7 dBu (LF), -1.7 dBu (HF)
* ISVPL threshold at 100 Vpk (LF), 50 Vpk (HF)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +10.2 dBu-pk (LF), +4.2 dBu-pk (HF)
* MaxPeak limiter threshold set 9 dB above MaxRMS, this should be adjusted down if ISVPL is not used