PLM series preset for passive Xo15 element.

-Application Notes
     2 way passive
     Xo15 used as monitor with Tk series Subwoofer
     Xover @ 100Hz
     Max 3 elements
     in parallel per channel

     (Additional Aux output for Br series).

-Routing
     Xo15 : 1 / 3
     Sub  : 2 / 4

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
     in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
