*** Tannoy VSX DR ***
___________________________________________

PLM & LM Series preset for Tannoy DIrect Radiating (DR) Subs
VSX 15DR, VSX 18DR
___________________________________________

Application Notes:

This 3 AUX module allows use of the separate Subwoofer
products for combination with suitable Full-Range Cabinets.

The X-over is set to 80Hz for use in combination with Lake/PLM/IPD VX Cut presets.
___________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***


::: Thomas Vestergaard :::
