Lab.gruppen's PLM Series preset suitable for JBL's VRX928LA speaker.

Application info:
VRX928LA single cabinet, active 2-way module.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +5 dBu (LF), -3 dBu (HF)
* ISVPL threshold at 87.1 Vpk (LF), 38.9 (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +9 dBu-pk (LF), +2 dBu-pk (HF)
* To emulate 26 dB Amp Gain - set input gain to -6 dB