*** Tannoy VSX8.2 CARDIOD SUB MODE ***
___________________________________________

PLM & LM Series preset for Tannoy VX 8.2 BP
For use in Cardiod Sub Configuration 
___________________________________________

Application Notes:

*** Configuration ***

Set the Subs lying horizontally one on top of the other.
Turn one of the subs round 180 degrees so the back is level with
the front of the other(s).

This Module has 3 Processed outputs:

1 = SUB : Low Frequency Driver
2 = SUB REAR : High Frequency Driver Compliment
3 = VX8 : For use of a VX8 Passive with the above Subs


These modules can be used in combination with other VX Module Files
should a different combination other than the VX8 within the module
be required.
___________________________________________

Routing:

Ensure The Front Facing subs are connected to the
correct channel/module output.
Ensure the Rear Facing Sub is connected to the correct
Channel/module output.

WARNING:: Ensure correct routing and cabling before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***
::: Thomas Vestergaard :::