Lab.gruppen's PLM Series preset suitable for L-Acoustics' ARCS II speaker

Application notes:
The module file is a 2-way configuration for full range application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), +2 dBu (HF)
* ISVPL threshold at 137.8 Vpk (LF), 69.1 Vpk (HF)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (LF), +7 dBu-pk (HF)
* MaxPeak limiter threshold set 9 dB above MaxRMS, this should be adjusted down if ISVPL is not used