Lab.gruppen's PLM Series preset suitable for JBL's SRX712M speaker.

Application notes:
The preset is for an actively driven speaker (Bi-Amp) in a two-way configuration.
This file will also work with stand alone Lake processors as long as 
32 dB gain is used in the amplifier.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10 dBu (LF), +1 dBu (HF)
* MaxPeak limiter threshold at +10.8 dBu-pk (=107 Vpk for LF), +1.0 dBu-pk (=52 Vpk for HF)
* ISVPL threshold set just above the MaxPeak thresholds
* To emulate 26 dB Amp Gain - set input gain to -6 dB

Fingerprint info:
SRX712M 1.1