PLM series preset for active Xo15 element.

-Application Notes
     2 way bi-amp
     Xo15 used as Front Of House system
     High Pass filter @ 70Hz
     Max 3 Xo15 elements
     in parallel per channel

     (Additional Aux output for Br series).

-Routing
     LF : 1 / 3
     HF : 2 / 4

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
     in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
