Lab.gruppen's PLM Series preset suitable for L-Acoustics' SYVA SUB speaker. v5.8

Application notes:
The preset is low-passed at 100 Hz, for use in combination with SYVA colinear line sources.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay, when using the channel SYVA SUB 3.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +6 dBu (SUB)
* ISVPL threshold at 150 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +12 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk