Adamson's PLM Series preset for Adamson's Metrix speaker and Metrix Sub

Application Notes:
     Preset used for 4 ways configuration 
     To be used with extra Subs LPF 60Hz
     Maximum of 6 Metrix cabinets in parallel per amplifier and 2 Metrix Sub (one per channel).

Routing:
     SUB 1 & 2 : 1 & 2
     LF/MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     V2.0 - 1 to 4 cabinets

Designed by DV2
Pascal GUILLAUME