Lake preset suitable for JBL's STX speakers.

Applications notes:
* LT = HF boost for Long Throw applications
* FR = Full Range / for combinations with subs ( with overlap ) 
* 80 = 80Hz CUT mode  / for combinations with subs ( no overlap ) 

Technical info:
* Amp Gain is 32 dB
* ISVPL threshold at 140.0 Vpk (SUB), 160.0 Vpk (LF), 47.0 Vpk (HF)
* To emulate 26 dB Amp Gain - set input gain to -6 dB