*** Turbosound PRAGUE TPA and TPZ Series ***
____________________________________________________

PLM & LM series modules:

TPA122/64/95/00, TPA152/64/95, TPZ122/64, TPZ152/64, TPZ153/64
____________________________________________________

Application Notes:

GAIN: all modules assume amplifier gain is 35dB.
For PLM this is already set and locked.
____________________________________________________

These models have 1, 2 or 3 processed output channels:
FR = Full Range (1 Channel)
FR + Sub = Full Range and Subwoofer (2 Channels)
Bi-amp Full Range (2 Channels)
Bi-amp + Sub (3 Channels)
Tri-amp (3 Channels Full range)
Tri-amp HP (3 Channels with high pass for sub integration)
Sub_Fullrange (subwoofer module for specific full range box)
____________________________________________________

Routing:

Any channel can be routed to the required output
from these modules.

WARNING: Ensure correct routing before use.
____________________________________________________      

*** Designed by Music Group ***

::: Andrew Pardoe 16/01/14 :::