*** TURBOSOUND FLASHLINE series 
______________________________________________________________
PLM & LM series modules:
TFS-500H, TFS-550L and suitable subwoofers 
______________________________________________________________
Application Notes:

GAIN: all modules assume amplifier gain is 35dB
For PLM this is already set and locked
Limiters are set in the modules
ISVPL where available is left open for
the user to further limit output if requried

DELAY: is set assuming cabinets are in line

Line array compensation: Modules are set up for 4 box line array
- For longer lines:
	increase highshelf, decrease lowshelf gains to suit
- For shorter lines
	decrease highshelf, increase lowshelf gains to suit
______________________________________________________________
Presets:

TFS-550H_SUB
- 2-Way module for use with subwoofers in a separate module

TFS-550H_550L 
- 3-Way module for TFS-550 H & L used together or as a
  4-way system with addition subwoofer in a separate module

SUBWOOFERS_550
- Separate module containing compatible subwoofers
  TFA-600L/B, TSW218, NuQ B18 
______________________________________________________________
Routing:

Any channel can be routed to the required output
from these modules.

WARNING: Ensure correct routing before use.
______________________________________________________________
*** Designed by Music Group ***

::: Andrew Pardoe 15/09/16 :::