*** TURBOSOUND MANCHESTER Series                             ***
***       V2.3 XP RELEASE                                    ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02 ***
*** All MODULES ARE CONTOUR XP FORMAT                        ***
***         README                                           ***

____________________________________________________
CHANGES: 

* DC VOCING OPTIMISATION all Arrays / Point Source V.2
** MC12-P OPTIMISATION OF MBL
*** isvlp OPTIMISATION UPDATE ALL MODELS
____________________________________________________

        HARDWARE LOCKING

ALL TURBOSOUND MANCHESTER SERIES LOUDSPEAKERS EXCLUSIVLY USE LAKE PRE-SETS VIA LAB.GRUPPEN PLM+ AND D SERIES L PLATFORMS. 
NO OTHER AMPLIFIER AND DSP PLATFORMS ARE SUPPORTED.

LM SERIES PROCESSORS ARE NOT COMPATIBLE WITH THESE MODULES.
TURBOSOUND MANCHESTER MODULES WILL NOT LOAD INTO LM SERIES PROCESSORS.
____________________________________________________
MODULE OUTPUT MIXING IS NOT REQUIRED FOR V2.3 XP RELEASE
V1.1 & V2.3 MODULES ARE NOT DESIGNED TO BE USED TOGETHER IN THE SAME SYSTEM

PLEASE CONSULT THE QUICK START GUIDE FOR DETAILED INSTRUCTIONS

____________________________________________________

All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02

*** Designed by TURBOSOUND - MAR 2024 ***
http://www.turbosound.com

