Tannoy's PLM Series preset suitable for Tannoy's VQ64DF speaker.

Application notes:
The preset is a 2-way configuration. A high pass filter 
(around 450 Hz, depending on the LF speaker) must be set for safe operation.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +2.0 dBu (MF), -1.0 dBu (HF)
* ISVPL threshold at 97.6 Vpk (MF), 69.0 Vpk (HF)