Tannoy's PLM Series preset suitable for Tannoy's VS15BP speaker.

Application notes:
The preset is a single channel configuration for this subwoofer, 
including a system hi-pass at 32 Hz (24 dB/oct Butterworth). 
It may require a low-pass crossover, to be set according to 
the main system specifications.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +5.0 dBu (SUB)
* ISVPL threshold at 138.1 Vpk (SUB)