Lab.gruppen's PLM Series preset suitable for L-Acoustics' KARA speaker

Application notes:
The module file is a 3-way configuration, designed for a downfill application 
flown underneath K1. This includes the optional SB18 in the module file.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +7.7 dBu (SUB), +4.7 dBu (LF), -1.7 dBu (HF)
* ISVPL threshold at 120 Vpk (SUB), 100 Vpk (LF), 50 Vpk (HF)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +11.8 dBu-pk (SUB), +10.2 dBu-pk (HF), +4.2 dBu-pk (HF)
* MaxPeak limiter threshold set 9 dB above MaxRMS, this should be adjusted down if ISVPL is not used