Tannoy's PLM Series preset suitable for Tannoy's VQ40/VS15DR speakers.

Application notes:
The preset is a 2-way configuration, with fixed crossover at 470 Hz 
between the LF section (VS15DR) and the Mid-High (VQ40). 
The LF section is high-passed at 40 Hz (12dB/oct Butterworth).

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10.0 dBu (VS15DR), +2.0 dBu (VQ40)
* ISVPL threshold at n/a (VS15DR), 97.6 Vpk (VQ40)