Adamson's PLM Series preset for Adamson's Metrix speaker and Metrix Sub

Application Notes:
     2 Metrix Wave stacked on MSUB 
     with Polemount Cabinet Harness

Routing:
     SUB 1 & 2 : 1 
     LF/MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     No

Designed by DV2
Pascal GUILLAUME