Lab.gruppen's PLM Series preset suitable for L-Acoustics' K1 speaker

Application notes:
The module file is a 3-way configuration for full range application.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8.3 dBu (LF), +8.3 dBu (MF), +1.8 dBu (HF)
* ISVPL threshold at 170 Vpk (LF), 120 Vpk (HF), 100 Vpk (HF)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +14.8 dBu-pk (LF), +11.8 dBu-pk (HF), +10.2 dBu-pk (HF)
* MaxPeak limiter threshold set 9 dB above MaxRMS, this should be adjusted down if ISVPL is not used