PLM series preset for active Xo15 element.

-Application Notes
     2 way bi-amp
     Xo15 used as monitor with Tk series
     Xover @ 100Hz

     (Additional Aux output for Br series).

-Routing
     Sub : 3 / 4
     LF  : 1
     HF  : 2

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
     in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
