Lab.gruppen's PLM Series preset suitable for L-Acoustics' dV-DOSC speaker.

Application notes:
Created for the "dV-DOSC 2W 60 HI" application;  
dV-DOSC (60 Hz HPF + LF shelving EQ) increased HF shelving EQ (bright).
Can be used with e.g. "SB218 60 Hz" provided that the delay and gain is tweaked.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +5 dBu (LF), +1 dBu (HF)
* ISVPL threshold at 97.6 Vpk (LF), 61.6 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +10 dBu-pk (LF), +6 dBu-pk (HF)

Fingerprint info:
dV-DOSC v1.0 beta1