*** Tannoy FIR VX6 CUT + VSX82 ***
___________________________________________

PLM Series FIR preset for Tannoy VX6 & VSX82
___________________________________________

Application Notes:

80Hz HPF CUT preset for use with VSX82 subwoofer.
Maximum of 4 cabinets in parallel per channel.
This is an FIR preset and requires 2 modules of DSP, A+B or C+D.
___________________________________________

Routing:

Channel 1 is VSX82
Channel 3 is VX6 CUT

Any channel can be routed to the required output from this module
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 5.8ms

Total system delay for this module is 6.35ms

___________________________________________

*** Designed by MUSIC TRIBE BRANDS Ltd ***


