*** TURBOSOUND BERLIN TBV Series ***
***   Constant Curvature Array   *** 
____________________________________________________

TBV123 2W BI-AMP + TBV118L 120 Hz 3-WAY FIR module

** This is an FIR preset, two modules of processing are required (A+B or C+D) **

OUTPUTS: 
Ch1=TBV118L 120 Hz LPF
Ch2=TBV123  LF FULLRANGE
Ch3=TBV123  HF

TBV123 pre-aligned for use with TBV118L front-firing subwoofers 
at 3:1 ratio but other TURBOSOUND subs can be used
____________________________________________________

EQ OVERLAYS:

- 2 BOX (nominal flat response for 2x TBV123)
- 3 BOX (nominal flat response for 3x TBV123)
- 4 BOX (nominal flat response for 4x TBV123)
- Long Throw (6 dB HF / 4 dB LF shelving applied)
____________________________________________________

Application Notes:

GAIN: all modules have 35 dB amplifier gain

PROCESSOR DELAY: 6.38ms

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TBV QSG and Rigging Manual prior to use 

*** Designed by Music Tribe Brands Ltd ***

