Lab.gruppen's PLM Series preset suitable for L-Acoustics' V-DOSC speaker.

Application notes:
Preset created for the "V-DOSC 3W HI" application;
V-DOSC (30 Hz HPF + LF shelving eq), increased HF shelving eq.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (LF), +9 dBu (MF), +9 dBu (HF)
* ISVPL threshold at 137.8 Vpk (LF), 154.8 Vpk (MF), 154.8 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (LF), +14 dBu-pk (MF), +14 dBu-pk (HF)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk