Lab.gruppen's PLM Series preset suitable for L-Acoustics' KS28 speaker. v5.8

Application notes:
The preset is low-passed at 100 Hz, for use in combination with large format line sources, e.g. K1 and K2 systems.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay, when using the channel KS28 3.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +7 dBu (SUB)
* ISVPL threshold at 137 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +12 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk