Lab.Gruppen (P)LM Series module preset suitable for TW AUDiO VERA20i speaker

Preset version: 3.11

Application notes:
* VERA20i in full-mode for stand-alone usage equipped with 120deg horn flares 
* Module contains two additional overlays with preconfigured filters: 
* 1. for array size correction - changing filter gain according to VERTICAL ARRAY CORRECTION section from preset guide
* 2 single - un-bypass filter when using a single cabinet

Technical info:
* Amp Gain is 32 dB
* Set MaxPeak Level to 3 dB for usage with PLM(+) Series
* Set MaxPeak Level to 0 dB for usage with LM44 or LM26

Support information:
* E-Mail:   support@twaudio.com
* Internet: https://twaudio.de/en/
* Phone:    +49 (0) 71 41 - 48 89 89 55

Compilation date: 04/12/2024