Lab.gruppen's PLM Series preset suitable for L-Acoustics' 12XT speaker.

Application notes:
The preset is designed for a fill application, high-passed at 100 Hz,
using the speaker in passive mode.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (Full-range)
* ISVPL threshold at 123.0 Vpk (Full-range)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (Full-range)